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	3D Stereoscopic Vision People Counter
3D PRO2TM













Product Code: FC-F3DP02



AI POWERED 3D STEREO VISION PEOPLE COUNTING
· Unparalleled Accuracy of Up to 99.5%
· Real-time Occupancy Counting
· Excellent Lifespan MBTF 25 years
· Bi-directional Counting
· Accurate Counting with Video Proof
· Superior Processing Power-Improved 3D Counting Accuracy

WIFI COUNTING
· Available metrics are outside traffic, visit duration, returning rate and traffic flow profiling.

STAFF EXCLUSION
· Staff are excluded from counting just by sewing, ironing or clipping the Staff Exclusion Tag on the shirt with no infrared or any emission involved.

OPTIMISED FOR ALL ENVIRONMENTS
· One lens fits all heights, caters for different types of stores with varying ceiling heights, as low as 2.1m to 4.5m. 
· Widest Coverage. Equipped with 160 degree dual fisheye lens, reduce the total number of counters required. 
· Superior Heat Dissipation. Enclosed in an aluminium unibody casing, prolong the lifespan of electronic components. 
· Low-light/ Night Mode Counting with External Infrared Light 
· Water Leakage-Proof. Enclosed in splash proof casing to reduce the counter failure rate due to the common issues like water leakage on the ceiling.

EASY TO INSTALL AND SET UP
· More Compact Form Factor 
· 1-year Manufacturer Warranty 
· GPIO Functionality. Integrate occupancy counting with all entrances and exits.




	




	TECHNICAL DATA
	

	
	
	Device Dimension (mm)
	154 (W) x 59 (D) x 40 (H)

	
	
	Packing Dimension (mm)
	200 (W) x 170 (D) x 50(H)

	
	
	Weight 
	Device: 0.4 kg   Packing: 0.86 kg 

	
	
	Camera
	2x 5MP, 160°, 5MP omni-vision 
5647 camera modules , RAM 1GB

	
	
	Illumination
	Minimum 1 lux (with external Infrared light source)

	
	
	Frame Rate
	25 fps (Live Stream of counting will only display 320x420 resolution to reduce bandwidth sent to database for verification purpose) 

	
	
	Indicator
	RGB LED status indicator

	
	
	Casing
	Made by Aluminium oxide alloy for dust resistance with 1mm tempered glass lens-covering. 

	
	
	IP Rating
	IP64

	
	
	Storage
	Built-in, 8 GB Storage

	
	
	Ideal Mounting Height
	2.1 metres – 4.5 metres

	
	
	Operating Environment
	Temperature 10°C to 45°C, Humidity 10% to 90%

	
	
	Storage Environment
	Temperature -40°C to 70°C, Humidity 10% to 95%

	
	
	Tracking Technology
	3D-Spacing Mapping Video Tracking Technology and background removal on static objects.

	
	
	Field Upgradable
	Manual / Auto Software upgrade

	
	
	Power Over Ethernet 
	Yes (IEEE802.3at)

	
	
	PoE Mode 
	Mode A/B

	
	
	Voltage
	8~56 VDC 

	
	
	Power Consumption
	6W

	
	
	Cabling
	Cat5e/Cat6, 100Mbps

	
	
	Origin
	Made in the UK

	
	
	
	

	
	
	  FIRMWARE SPECIFICATION FOR DEVICE LEVEL

	
	
	Interface
	Http; Https

	
	
	User Levels
	2 levels: Administrator, 
Standard Usery

	
	
	Operating System
	Footfall Counter OS

	
	
	Ethernet
	10/100 Mb Ethernet

	
	
	Data Delivery
	TCP/IP

	
	
	Database Type 
	SQLite

	
	
	Report Format
	csv, .xml, .txt

	
	
	Data Storage on 
counter level 
	Hourly Data: 300 days; Raw Data: 7 days; 3 days *Data which has sent to server will keep permanently in server level

	
	
	Data Backup
	Yes

	
	
	Firmware Feature
	Secure Operating System with Multicore Processor, Adaptive IR based on Lighting Conditions, Device Health Check, Built-in External Watchdog

	
	
	Data Upload to Server
	Every Hour

	
	
	Average Data Transfer Rate*
	10.0 kilobytes/hour

	
	
	*Average Data Transfer Rate is measured with a predefined sample size of 20 requests per hour






PRODUCT DIMENSION
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COVERAGE TABLE
	Ceiling Height (m)
	Lens Degree
	Coverage Area (m) 
(Horizontal FOV x Vertical FOV)

	2.1 
	160 
	1.57 x 1.17 m

	2.5
	160 
	2.62 x 1.96 m

	3.0
	160 
	3.94 x 2.93 m

	3.5
	160 
	5.25 x 3.91 m

	4.0
	160 
	6.56 x 4.89 m 

	4.5
	160 
	7.08 x 5.28 m



Notes: 
1. For mounting height >4.50m, please contact sales@footfallcam.com for another mode recommendation of FootfallCam. 
2. For mounting height >8.00m, recommend to use drop pole when installing the counter to the acceptable range


Do you need further information or have a question? Please visit www.footfallcam.com
©2002-2023 Footfall counter is trademark application of FootfallCam in various jurisdictions. We reserve the right to introduce 
modifications without notice. All other company names and products are trademarks of their respective companies. 
Do you need further information or have a question? Please visit www.footfallcam.com
©2002-2023 Footfall counter is trademark application of FootfallCam in various jurisdictions. We reserve the right to introduce modifications without notice. All other company names and products are trademarks of their respective companies. 
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