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Product Code: FC-FCT01



KEY FEATURES
· Real time processing data
· Designed for human and vehicle detection
· Process up to eight HD full-motion video streams
· Low-power edge intelligent video analytics
· FootfallCam Centroid works in conjunction with FootfallCam people counter and/or any CCTV cameras
· Data Metrics involved in the FootfallCam people counter can be computed by FootfallCam Centroid

MULTI STREAM VIDEO ANALYSIS
· Can be connected to up to 8 CCTV cameras for maximum coverage and cost-effectiveness. The videos from PoE Switch/ DVR/ NVR are processed in real time to generate in-depth data analytics. The aggregated data from each raw video stream are available to be accessed through FootfallCam Analytic Manager V9™ with read-made modules and reports.

OBJECT DETECTION (LOCALIZATION)
· Powerful processor to deploy as a low-power edge intelligent video analytics platform for Network Video Recorders (NVR), smart cameras and IoT gateways. FootfallCam Centroid™ carries out object detection and classification for any industry.

CCTV REQUIREMENTS
· Compatible processing data through Real time Streaming Protocol (RTSP) 
· Allow direct video stream from RTSP enabled IP Cameras 
or Network Video Recorders (NVR)
· Installed between 2 to 6 metres ceiling height with ideal mounting height between 3 to 4 metres.
· No distortion / fisheye lens on the analytic zone
· Minimum video resolution of 720p
· Minimum video frame rate of 10fps


	




	GENERAL SPECIFICATION

	
	
	Model
	Centroid

	
	
	Weight
	270 gm

	
	
	Casing Colour
	Black

	
	
	Casing Material
	Metal

	
	
	Total Dimensions (mm)
	104 (W) x 81 (D) x 60 (H)

	
	
	Warranty
	1 year from first allocation date (Warranty extension available upon request)

	
	
	CPU
	64-bit Quad-core @ 1.43GHz

	
	
	GPU
	128-core @ 921MHz

	
	
	Memory
	4GB 64-bit LPDDR4 @ 1600MHz | 25.6 GB/s

	
	
	Video Encoder
	4Kp30 | (4x) 1080p30 | (2x) 1080p60

	
	
	Video Decoder
	4Kp60 | (2x) 4Kp30 | (8x) 1080p30 (4x) 1080p60

	
	
	Processor Power
	10W

	
	
	USB
	4x USB 3.0 A (Host) | USB 2.0 Micro B (Device)

	
	
	Display
	HDMI | DisplayPort

	
	
	Networking
	Gigabit Ethernet (RJ45)

	
	
	Wireless
	M.2 Key-E with PCIe x1

	
	
	Storage
	MicroSD card (16GB UHS-1 recommended minimum)

	
	
	Other I/O
	(3x) I2C | (2x) SPI | UART | I2S | GPIOs

	
	
	Power Supply
	5V4A DC Power Adapter

	
	
	Average Data Transfer Rate*
	5.0 kilobytes/hour

	
	
	* Average Data Transfer Rate is measured with a predefined sample size of 20 requests per hour.



	
	
	

	
	
	
	

	
	
	PRODUCT DIMENSION
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Do you need further information or have a question? Please visit www.footfallcam.com
©2002-2023 Footfall counter is trademark application of FootfallCam in various jurisdictions. We reserve the right to introduce 
modifications without notice. All other company names and products are trademarks of their respective companies. 
Do you need further information or have a question? Please visit www.footfallcam.com
©2002-2023 Footfall counter is trademark application of FootfallCam in various jurisdictions. We reserve the right to introduce modifications without notice. All other company names and products are trademarks of their respective companies. 
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